**Havnehusene**

**The SALTO chip**

**How to use**

1. When using the chip it has to hold on the reader.
2. If the wall reader blinks blue the chip cannot be removed before the reader blinks green and gives a beep.
3. If the reader blinks red and beeps you do not have the authorization to open the door.
4. If the reader blinks green and beeps the door will unlock and you will have 10 seconds to get before the door locks again, the reader again will blink red with a beep, and the door once again be locked.
5. If the reader blinks green 3 times accompanied with longer beeps the door is unlocked, and the door will stay unlocked for a certain amount of time or the chip is once again placed on the reader.

The reader will now give a red blink accompanied by a beep and the door is again locked.

Good luck with your new access control